,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Sanesca W2 LED2600-830 ET 01,0.7,0.19,0.09,10117155,6337440,2,Verkehrsweiß RAL 9016,4.4,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6337440,Schutzklasse I,,ET,LED,47.5,80,4596,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_3000_Sanesca,Sanesca_LS : TX040695
