,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Arimo M46 RAV LED4500-840 ET 01,1.197,0.297,0.051,50254078,7845740,RAL9016 Verkehrsweiß ,4.7,http://www.trilux.com/TOC/7845740,I,IP20,ET,LED,36,80,54 84 98 100 100,4500,4000,TRILUX_RAL9016,TRILUX_WH_4000,ArimoRAV_LS : TX277665
Arimo M46 RAV LED4500-840 ETDD 01,1.197,0.297,0.051,50254077,7845751,RAL9016 Verkehrsweiß ,4.7,http://www.trilux.com/TOC/7845751,I,IP20,ETDD,LED,37,80,54 84 98 100 100,4500,4000,TRILUX_RAL9016,TRILUX_WH_4000,ArimoRAV_LS : TX277667
Arimo M57 RAV LED4500-840 ET 01,1.247,0.309,0.051,50254076,7845640,RAL9016 Verkehrsweiß ,4.8,http://www.trilux.com/TOC/7845640,I,IP20,ET,LED,35,80,54 84 98 100 100,4500,4000,TRILUX_RAL9016,TRILUX_WH_4000,ArimoRAV_LS : TX277666
Arimo M57 RAV LED4500-840 ETDD 01,1.247,0.309,0.051,50254075,7845651,RAL9016 Verkehrsweiß ,4.8,http://www.trilux.com/TOC/7845651,I,IP20,ETDD,LED,37,80,54 84 98 100 100,4500,4000,TRILUX_RAL9016,TRILUX_WH_4000,ArimoRAV_LS : TX277664
