,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Ref##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
7651IP HE LVN 40-830ET L150 01,1.474,0.063,0.062,10245401+10241408,9002114330+7789600,RAL9016 Verkehrsweiß,0,http://www.trilux.com/TOC/9002114330,I,IP50+IP50,ET,LED,22,80,86 96 99 99 100 0 0 36 1,4000,3000,7651_IP50_L,TRILUX_RAL9016,TRILUX_WH_3000,7651_LS : TX264792
