,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Faciella Slim 40 AM17R/5100-830 1G1 ETDD,0.102,0.368,0.365,10206611,7396651,DB703 Anthrazit,5.3,http://www.trilux.com/TOC/7396651,I,IP65,ETDD,LED,80,80,32 70 96 100 100,5100,3000,TRILUX_DB703,TRILUX_WH_3000,Faciella_Slim_LS : TX120356
