,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Faciella Slim 30 RE5R/2000-830 3G1 ETDD,0.102,0.268,0.256,10206597,7395251,DB703 Anthrazit,3.3,http://www.trilux.com/TOC/7395251,I,IP65,ETDD,LED,40,80,96 98 99 100 99,2000,3000,TRILUX_DB703,TRILUX_WH_3000,Faciella_Slim_LS : TX120344
