,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,ref_array##OTHER##,Light Source##OTHER##
Actison Fit D1 CDP 9300-840 ETDD,1.548,0.31,0.095,10210412,7427951,RAL9016 Verkehrsweiß,11.3,http://www.trilux.com/TOC/7427951,I,IP20,ETDD,LED,69,80,65 90 98 100 100,9.300,4000,TRILUX_RAL9016,TRILUX_WH_4000,1,Actison_Fit_LS : TX113437