,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Light Source##OTHER##
Mirona Fit-TP TB LED40000-840 ETDD,0.649,0.559,0.065,10142516,6821551,Mirona_Fit_GH : 6_LED_Module,Verkehrsweiß RAL 9016,12,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6821551,Schutzklasse I,IP65,ETDD,LED,282,80,39486,4000,Mirona_Fit_LS : TX050486
