,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SEO_outer##OTHER##,cutout_radius##LENGTH##METERS,Light Source##OTHER##
Inplana C09 OTA25 3000-830 ET 01,0.316,0,0.041,10130573,6455740,Inplana_C09,RAL9016 Verkehrsweiß,1.43,http://www.trilux.com/TOC/6455740,II,IP20,ET,LED,24,80,52 83 96 100 100 0 0 0 0,3000,3000,TRILUX_RAL9016,TRILUX_WH_3000,TRILUX_CDP_Inplana_WH_outer_3000,0.150,Inplana_LS : TX049212
