,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Cultega Act T SMC PAW 600 ETDI 01(ACTDSU),0.135,0,0.025,10255769,7854759,RAL9016 Verkehrsweiß,4.71,http://www.trilux.com/TOC/7854759,II,IP20,ETD,LED,7.9,90,54 85 97 100 100,650,4000,TRILUX_RAL9016,TRILUX_WH_4000,Cultega_LS : TX280866
