,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Valineo G3 M73 PW19 40-830 ET, 0.595, 0.595, 0.0135,10223336,7570140,RAL9016 Verkehrsweiß, 2.1,http://www.trilux.com/TOC/7570140,II,IP20,ET,LED,34,80,65 88 97 100 100 0 0 0 0,4000,3000,TRILUX_RAL9016,TRILUX_WH_3000,Valineo_G3_LS : TX149762
