,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Cultega Act T COM PAW 600 ETDI KL 01(ACTDCW),0.135,0,0.025,10255775,7916259,RAL9016 Verkehrsweiß,4.71,http://www.trilux.com/TOC/7916259,II,IP20,ETDD,LED,7.2,90,54 85 97 100 100,650,6300,TRILUX_RAL9016,TRILUX_WH_6300,Cultega_LS : TX280851
