,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Light Source##OTHER##,Mat##OTHER##,SEO##OTHER##,Polaron_GH##OTHER##
PolaronIQ WD2D LED3000-840 ETDD,0.4,0,0.068,10138738,6671551,TRILUX_WH_4000,RAL9016 Verkehrsweiß,3.05,http://www.trilux.com/TOC/6671551,I,IP40,ET,LED,27,80,31 59 83 80 100 11 34 64 20,3100,4000,PolaronIQ_LS : TX049145,TRILUX_RAL9016,TRILUX_WH_4000,PolaronIQ_WD1_WD2
